Software description

1. Installs
   1. Windows 7
   2. TesterXpWin7\_3.4 (TclTk8.6, RLSerial, RLExPio, RLEtxGen, RLTime, RLStatus, RLSound)
2. AT software package
   1. C:\ETX-220A-MP
3. Operation files
   1. Tester1\_Etx220AMP.tcl, Tester2\_Etx220AMP.tcl, Tester3\_Etx220AMP.tcl, Tester4\_Etx220AMP.tcl, Tester5\_Etx220AMP.tcl, Tester6\_Etx220AMP.tcl, Tester7\_Etx220AMP.tcl, Tester8\_Etx220AMP.tcl

The Tester performs DDR test of the ETX220-A-MP. The checking is performing by power OFF and ON and then reading the UUT’s log.

The HW definitions – COM and PIO ports – are defined in HWinit.tcl file, which located at folder C:\ETX-220A-MP\[PC name]. The [PC name] is defined by [info host].